**CORRIGENDUM I**

**Name of work : Additional Civil & electrical works in the New Condom manufacturing facility at Rubber Park, Irapuram, Kochi**

**Tender no. HLL/ID/13/79 dtd 01.10.2013**

The description for item no. 12 (a) in Civil works & 5 (b) in Appendix A (of civil works) may please be read as follows:

|  |  |  |
| --- | --- | --- |
| **Item no.** | **Original specification** | **Amended** |
| 12 (a) | Reinforcement cement concrete work in walls (any thickness) including attached pilasters, buttresses, plinth and string courses. Fillets, columns, pillars, piers, abutments, posts and struts, etc. upto floor five level including cost of centering, shuttering , strutting, propping etc and removal of formwork, finishing and reinforcement.1:1.5:3 (1 cement : 1.5 coarse sand : 3 graded stone aggregate 20 mm nominal size.) Lintels, weather shade, chajja, Foundations of machines etc | Reinforced cement concrete work in walls (any thickness) including attached pilasters, buttresses, plinth and string courses. Fillets, columns, pillars, piers, abutments, posts and struts, etc. upto floor five level **excluding**  cost of centering, shuttering, strutting, propping etc and removal of formwork, finishing and reinforcement. 1:1.5:3 (1 cement: 1.5 coarse sand: 3 graded stone aggregate 20 mm nominal size.) Lintels, weather shade, chajja, Foundations of machines etc |
| 5(a) | Reinforcement cement concrete work in walls (any thickness). including attached pilasters, buttresses, plinth and string courses. Fillets, columns, pillars, piers, abutments, posts and struts, etc. upto floor five level including cost of centering, shuttering, strutting, propping etc and removal of formwork, finishing and reinforcement.1:1.5:3 (1 cement : 1.5 coarse sand : 3 graded stone aggregate 20 mm nominal size.) Lintels, weather shade, chajja etc | Reinforced cement concrete work in walls (any thickness) including attached pilasters, buttresses, plinth and string courses. Fillets, columns, pillars, piers, abutments, posts and struts, etc. upto floor five level **excluding** cost of centering, shuttering, strutting, propping etc and removal of formwork, finishing and reinforcement.1:1.5:3 (1 cement : 1.5 coarse sand : 3 graded stone aggregate 20 mm nominal size.) Lintels, weather shade, chajja etc |

Deputy Vice President (Techncial)