**20.01.2014**

|  |
| --- |
| **Amendment -III****Tender No. HLL/ID/14/02 Dated: 03.01.2014** |
| **Sub: Construction of 2 Doctors Dispensary at Vadavathoor, Kottayam for ESIC** **The quantity of the following items for the Civil Works (Part –I) is to be read as follows: (No change in estimate cost put to tender)**

|  |  |  |  |
| --- | --- | --- | --- |
| **ITEM NO** | **DESCRIPTION** | **QUANTITY** | **UNIT** |
| 2 | Filling available excavated earth (excluding rock) in trenches, plinth, sides of foundations etc. in layers not exceeding 20 cm in depth :consolidating each deposited layer by ramming and watering,lead up to 50 mm and lift upto 1.5m | 339.65 | CUM |
| 4 | Supplying and filling in plinth with river sand/quarry dust under floors including,watering consolidating and dressing complete. | 72.27 | CUM |
| 5 (b) | Providing and laying in position cement concrete of specified grade excluding the cost of centring and shuttering - All work upto plinth level | 72.27 | CUM |
| 6 | Applying a coat of residual petroleum bitumen of grade of VG-10 of approved quality using 1.7kg per square metre on damp proof course after cleaning the surface with brushes and finally with a piece of cloth lightly soaked in kerosene oil. | 75.07 | SQM |
| 8 (e) | Centring and shuttering including strutting, propping etc. and removal of form for: Stairs,(excluding landings) except spiral-staircasess. | 16.80 | SQM |
| 9 (a) | Steel reinforcement for R.C.C. work including straightening, cutting, bending, placing in position and binding all complete upto plinth level. | 9711.67 | KG |
| 9 (b) | Steel reinforcement for R.C.C. work including straightening, cutting, bending, placing in position and binding all complete upto plinth level. | 20266.22 | KG |
| 10 (a) | Providing and laying in position machine batched and machine mixed design mix M-25 grade cement concrete for reinforced cement concrete work -------- | 74.71 | CUM |
| 10 (b) | All works above plinth level upto floor V level. | 155.89 | CUM |
| 12 | Brick work in superstructure above plinth level upto floor V level in cement mortar 1:6. | 198.76 | CUM |
| 15 | Providing and fixing dry cladding upto 10 metre heights with 30mm thick gang saw cut stone with (machine cut edges) of uniform colour and size upto 1mx1m ------ | 440.21 | SQM |
| 16 | Providing and fixing structural steel frame (for dry cladding with 30 mm thick gang saw cut with machine cut edges sand stone) on walls at all heights using M.S. square/ rectangular tube in the required pattern as per architectural drawing including cost of cutting, bending, welding etc.  | 3521.68 | KG |
| 17 | Providing and fixing adjustable stainless steel cramps of approved quality and of required shape and size adjustable with stainless steel nuts, bolts and washer (total weight not less than 260 gms) for dry stone cladding fixed ------- | 1320.00 | EACH |
| 19 | Stone tile (polished) work for wall lining over 12mm thick bed of cement mortar 1:3 (1 cement : 3 coarse sand) and cement slurry @ 3.3 kg/sqm including pointing in white cement complete. 8mm thick. Granite of any colour and shade. | 1109.52 | SQM |
| 31 | Providing and fixing Ist quality ceramic glazed wall tiles (Light Blue) conforming to IS : 15622 (thickness to be specified by the manufacture of approved make in all colours, shades except burgundy, bottle green, black of any size as approved by Engineer-in-Charge ---- | 82.07 | SQM |
| 32 | Providing and laying rectified Glazed Ceramic floor tiles 300 X300 mm or more(thickness to be specified by the manufacturer) of 1st quality conforming to IS : 15622 of approved make in colours White, lvory, Grey , Fume Red Brown laid on 20 mm thick Cement Mortar 1:4 (1 Cement : 4 Coarse sand ) including grouting the joints with white cement and matching pigments etc., complete.(SOMANY RUSTICO AZURE TILES 300 X300 MM) | 29.61 | SQM |
| 37 | Providing and fixing false ceiling with 12 mm thick plain/ semi perforated or with design ceiling tiles of BWP type phenol formaldehyde synthetic resin bonded pressed particle board conforming to IS:3087, finished with a coat of aluminium primer on both sides & ---  | 301.95 | SQM |
| 38 | Providing and fixing tiled false ceiling of approved materials of size 595x595 mm in true horizontal level suspended on inter locking metal grid of hot dipped galvanized steel sections ------ | 129.41 | SQM |
| 39 | 12mm cement plas 1:6 ( 1 cement : 6 fine sand)ter of mix: | 1100.56 | SQM |
| 40 | 15 mm cement plaster on the rough side of single or half brick wall of mix: 1:6(1 cement : 6 fine sand) | 1092.29 | SQM |
| 41 | Distempering with oil bound washable distemper of approved brand and manufacture to give an even shade: New work ( two or more coats ) over and including priming coat with cement primer | 1100.56 | SQM |
| 42 | Painting with synthetic enamel paint of approved brand and manufacture to give an even shade Two or more coats on new work | 61.10 | SQM |
| 43 | Applying priming coat with ready mixed aluminium primer of approved brand and manufacture on resinous wood and ply wood | 61.10 | SQM |
| 44 | Finishing walls with textured exterior paint of required shade: | 440.21 | SQM |

**The amendment forms part of tender document and has to be submitted along with the tender duly signed.****Deputy Vice President (Technical)** |
|  |
|  |
|  |
|  |
|  |  |  |  |  |

**Deputy Vice President (Technical)**

**HLL Lifecare Limited**

**Infrastructure Development Division**