|  |  |  |
| --- | --- | --- |
| Sl No | Original as per tender | Amended Specification  |
| 1 | **Torch- Local Purchase** |

|  |
| --- |
| LED type torch |
| Should be supplied with rechargeable batteries and charger |
| Should be suitable for clinical application |

 |
| 2 | **Vacuum Cleaner- Local Purchase** |

|  |
| --- |
| Should have minimum 1200 Watts of Powerful Suction |
| Blower efficiency 30-35lt/sec |
| Should be suitable for wet and dry application |
| Power supply: 230V,50 Hz |

 |
| 3 | **Oxygen Cylinder With Gauge- Local Purchase** |

|  |
| --- |
| Should be type B oxygen cylinder with regulator and gauge |
| Should be with oxygen flow meter with humidifier bottle attached to the regulator |
| Should be supplied with portable oxygen trolley made up of MS |

 |
| 4 | **Cidex Tray- Local Purchase** |

|  |
| --- |
| Should be made up of polypropylene |
| Heat resistant up to 134 degree Celsius |
| Approximate Dimension : 750 mm X 220 mm X 130mm ( 14 litres) |
| Should be supplied with lid  |

 |
| 5 | **Emergency Lamp- Local Purchase** |

|  |
| --- |
| Should be rechargeable emergency light  |
| Brightness should be 1000 lumens or more |
| Should provide minimum 4 hours back up  |
| Should be LED based or CFL based  |
| Should be supplied with all accessories |

 |