Amendment / Corrigendum to Tender

Sub: TENDER FOR ESTABLISHMENT OF DEIC AT KNH SHIMLA

IN THE STATE OF HIMACHAL PRADESH ON TURNKEY BASIS.

Ref: **IFB NO: HLL/AFT-CMO/HP-DEIC/EQP/2017-18 DATED 14.02.2018**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sl No** | **Instead of** | | | **Read as** | |
| 1. | RET cam or any other Camera to take photographs of the fundus of the new-born | | | Portable Modular Retinal Camera for Premature Babies (ROP) | |
| **CORRIGENDUM / AMENDMENT TO SECTION VI-Technical Specification (Page – 119)** | | | | | |
| SPECIFICATIONS PORTABLE MODULAR RETINAL CAMERA FOR PREMATURE BABIES  ( ROP Device)   * It should be Light weight and portable modular retinal camera for diagnosis of retinal diseases of the premature babies. * Minimum 120 degree field of view. * Should be able to capture images of the entire eye in a video mode and should be convertible to an image mode for email. * Retinal camera should be tele medicine compatible so that the high quality and high resolution images of the infant eye could be shared with anyone anywhere for views. * Software should support sending and receiving images and diagnosis. * Should have high quality image editing tool to convert the film clip of the screening to frames and freedom of selecting frames. * Should also assist in image enhancement and compression for faster and efficient transmission. * Should have adjustable intensity, gain, balance, brightness, contrast, and gamma. * Should be compatible with DICOM export, Telemedicine, USB 3.0, MS WINDOW 8.1 or better. * Image resolution ------ 2040x2040-24 bit colors. * Should be able to measure pupil size of 4mm and above. * Minimum 120 degree field of view from center of the eye. * Should supplied with branded laptop with following specification   + High Speed i5 Processor or higher, RAM 8GB or more, Hard disk -1 TB or more, Window 8.1 or better, Display at least 15 inch or more | | | | | |
| **Sl No** | | | **Original Tender Details** | **Amended Tender Details** | |
| 1. | | | **Bid Submission Closing Date**  28/02/2018 at 14.00 hrs  **Bid Opening Date**  28/02/2018 at 15.00 hrs | **Bid Submission Closing Date**  05/04/2018 at 14.00 hrs  **Bid Opening Date**  05/04/2018 at 15.00 hrs | |

All other terms and conditions in the original tender remain unchanged.

**21-03.2018                                                            Joint General Manager (Materials)**